Ic7 Adressmap	All real text can be changed!

		H= hexidecimal( 0 1 2 3 4 5 6 7 8 9 a b c d e f  -10 11and so on) 
		D= decimal. ( 0 1 2 3 4 5 6 7 8 9 10)      

Presets starting at 16000 H end at 1a69a H

Registration Bank Presets 38 pcs.
Preset1: 		16112 H -  1614e H

Reset Bank Presets 16D pcs.
Preset1:        	1a22d H -  1a26a H  61 D adresser
Preset16:       stops with  1a69a H    
The in between adresser are intern hs8 parameters                

Voices start from 1cb00 H  end at 1ebff H
LowerCombVoice1:	1cc51 H	-   1cc8a H
RegistMenuCombi1:	1d102 H -   1d13a H

Adesses ae indicative only!
Please email me expandings of map!