Yamaha MU100R

Ver1.05 97-Sep-19

Ver1.06 97-Oct-14

Ver1.11 99-Aug-03

Sticker v1.06
~~~~~~~~~
 (c)1997
 Yamaha
 XT714
  H0
~~~~~~~~~

2012/11/20

Endinanness in your programming tools may be reversed.
To ensure that what you burn matches the necessary endianness, you'll have to read out
the old rom from your device through your tools and compare byte sequence with this one.
Swap bytes if necessary, and then burn that data.


Edward d-tech
www.dtech.lv
